(footprint "rp2040zero_upside_down"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "U1"
		(at 7.6 2.72 0)
		(unlocked yes)
		(layer "B.SilkS")
		(uuid "a9268a53-a12f-4d94-a4e2-fb44996be93e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
			(justify mirror)
		)
	)
	(property "Value" "~"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "ba3bc424-cb10-4a20-9a15-569e4bb2ecbf")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "cmdr-joystick:rp2040zero_upside_down"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "740392c5-927e-455b-bf30-349f7c7d9c97")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "50300cc0-6346-4e2b-9337-4a2b58a4834a")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "66873f71-c95e-4279-997c-798e5c787d04")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "06527dec-6380-4372-be80-301d8dc131ca")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole rect
		(at -7.62 5.08)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "17947267-dced-4076-9b2f-347ddc8b4198")
	)
	(pad "2" thru_hole circle
		(at -7.62 7.62)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f41e9c75-62c9-4146-a361-dcef9b889614")
	)
	(pad "3" thru_hole circle
		(at -7.62 10.16)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "8a2f8450-c7ee-42e9-beaa-80ca47b61325")
	)
	(pad "4" thru_hole circle
		(at -7.62 12.7)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "e2ffab03-f905-42ee-8780-5b06029fabfa")
	)
	(pad "5" thru_hole circle
		(at -7.62 15.24)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "4da7e2c7-cc48-4e24-ab42-9eda715b69f4")
	)
	(pad "6" thru_hole circle
		(at -7.62 17.78)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "43bbe4ec-02e3-4ca0-9dcf-cfbf014c63f0")
	)
	(pad "7" thru_hole circle
		(at -7.62 20.32)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f8050ea6-5f8f-42e3-a134-88bb611270b2")
	)
	(pad "8" thru_hole circle
		(at -7.62 22.86)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "97f2a286-24e2-4e52-814e-b7200c8be051")
	)
	(pad "9" thru_hole circle
		(at -7.62 25.4)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "d633218d-0d26-4609-99cf-4f9cf8859ecd")
	)
	(pad "10" thru_hole circle
		(at -5.08 25.4)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "0d06bef7-c329-4b1a-a9ba-b4d019d52d26")
	)
	(pad "11" thru_hole circle
		(at -2.54 25.4)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "8419f4c0-031f-4074-a434-b41d1176538b")
	)
	(pad "12" thru_hole circle
		(at 0 25.4)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "5abc5c69-fcf6-4137-87f8-dc9027449bb1")
	)
	(pad "13" thru_hole circle
		(at 2.54 25.4)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a5a3e7a5-d7d8-4899-abdd-c897c28505cf")
	)
	(pad "14" thru_hole circle
		(at 5.08 25.4)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "da2afb69-f16a-4007-bac5-ba3bcb158726")
	)
	(pad "15" thru_hole circle
		(at 7.62 25.4)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "0fa419ab-644c-4076-9545-7321d785f0af")
	)
	(pad "16" thru_hole circle
		(at 7.62 22.86)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f8885244-66bd-4586-b9a1-8505777af91d")
	)
	(pad "17" thru_hole circle
		(at 7.62 20.32)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "98ce0929-290b-48df-a6ec-68d9c9915828")
	)
	(pad "18" thru_hole circle
		(at 7.62 17.78)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "6c138d01-e6db-4129-b486-27d0fdbe007f")
	)
	(pad "19" thru_hole circle
		(at 7.62 15.24)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "7ff4530b-c77b-4fa3-bc58-0ec0634b435b")
	)
	(pad "20" thru_hole circle
		(at 7.62 12.7)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "9b43863f-cc2f-41bc-8939-c2182fb32c91")
	)
	(pad "21" thru_hole circle
		(at 7.62 10.16)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "5650fc77-cfb7-42bd-bd6d-3f26d85fd2a5")
	)
	(pad "22" thru_hole circle
		(at 7.62 7.62)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "ca1c667b-3e9c-4b34-aba8-c9786a8ffcbe")
	)
	(pad "23" thru_hole circle
		(at 7.62 5.08)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "6c1fc3f1-668f-43d1-a384-e3e89046558f")
	)
	(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x09_P2.54mm_Vertical.wrl"
		(offset
			(xyz -7.5 -25.5 -4)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -180 -180 0)
		)
	)
	(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x09_P2.54mm_Vertical.wrl"
		(offset
			(xyz 7.5 -25.5 -4)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 -180)
		)
	)
	(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
		(offset
			(xyz 5 -25.5 -4)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -180 -180 -90)
		)
	)
	(model "${KIPRJMOD}/RP2040_Zero.stp"
		(offset
			(xyz 9 -27 -5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 -180 0)
		)
	)
)
