(module FRJAE-408 (layer F.Cu) (tedit 5E407110)
  (descr "8 Pol Shallow Latch Connector, Modjack, RJ45 (https://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/c-bmj-0102.pdf)")
  (tags RJ45)
  (fp_text reference J1 (at -4.505 7.747 180) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value RJ45 (at 4.445 4 180) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 4.445 2 180) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -4 0.5) (end -3.5 0) (layer F.SilkS) (width 0.12))
  (fp_line (start -4 -0.5) (end -4 0.5) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.5 0) (end -4 -0.5) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.205 8.382) (end -3.205 -2.77) (layer F.Fab) (width 0.12))
  (fp_line (start 12.095 8.382) (end -3.205 8.382) (layer F.Fab) (width 0.12))
  (fp_line (start 12.095 -3.77) (end 12.095 8.382) (layer F.Fab) (width 0.12))
  (fp_line (start -2.205 -3.77) (end 12.095 -3.77) (layer F.Fab) (width 0.12))
  (fp_line (start -3.205 -2.77) (end -2.205 -3.77) (layer F.Fab) (width 0.12))
  (fp_line (start -3.302 8.382) (end 12.218 8.382) (layer F.SilkS) (width 0.12))
  (fp_line (start 12.205 -3.88) (end 12.205 8.382) (layer F.SilkS) (width 0.12))
  (fp_line (start 12.205 -3.88) (end -3.315 -3.88) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.315 -3.88) (end -3.302 8.382) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.71 -4.27) (end 12.6 -4.27) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.71 -4.27) (end -3.71 14.47) (layer F.CrtYd) (width 0.05))
  (fp_line (start 12.6 14.47) (end 12.6 -4.27) (layer F.CrtYd) (width 0.05))
  (fp_line (start 12.6 14.47) (end -3.71 14.47) (layer F.CrtYd) (width 0.05))
  (pad "" np_thru_hole circle (at 10.16 6.35) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at -1.27 6.35) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  (pad 1 thru_hole rect (at 0 0) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 1.27 -2.54) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 2.54 0) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 3.81 -2.54) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 5.08 0) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at 6.35 -2.54) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask))
  (pad 7 thru_hole circle (at 7.62 0) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask))
  (pad 8 thru_hole circle (at 8.89 -2.54) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask))
  (model ${KIPRJMOD}/FRJAE-408.step
    (offset (xyz 4.5 -14.5 13))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
