{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["RF-Chip","Ordlista","Regler"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"RF-Chip","index":0,"n_rows":13,"n_cols":18,"rows_kept":13,"flags":["formulas_cached_only"]}
["Fabrikat","Modell","Ordering PartNr/Kapsel","MCU","Band (MHz)","i Rx/Tx (mA)","i Stnd By (nA)","VDD (V)","Modulering","Modell","P Tx (dBm)","Mott.känslighet","Kanalsep","Baudrate (kbps)","Interface","Xtal (MHz)","Features","Pris"]
["Nordic Semicon","nRF905","nRF905 / (QFN32L)","N","433 / 868 / 915","12,5 / 30",2500,"1,9 - 3,6","GFSK","nRF905","+10 adjust","-100","100kHz","50","SPI","4 - 20","Carrier detect"]
["Nordic Semicon","nRF9E5","nRF9E5 /  (QFN32L)","J","433 / 868 / 915","12,5+1/",2500,"1,9 - 3,6","GFSK","nRF9E5","+10 adjust","-100","100kHz","50","SPI","4 - 20","Carrier detect"]
["Chipcon/Texas","cc400","CC400-RTB2","N","300 - 500","23 / 77 (14dBm)",200,"2,7 - 3,3","FSK","cc400","-5 +14","-110","10kHz","9,6","3-wire serial",12]
["Chipcon/Texas","cc900","CC900","N","800 - 1000","21 / 91",200,"2,7 - 3,3","FSK","cc900","-20 +4","-110","10kHz","9,6",null,12]
["Chipcon/Texas","cc1000","CC1000","N","300 - 1000","7,4 / 26,7",200,"2,1 - 3,6","FSK/OOK","cc1000","-20 +10","-110 (2,4kbps)","65kHz","76,8","3-wire serial",14.7456,"Programable Xtal tempcorrection"]
["Chipcon/Texas","cc1010","CC1010-STY1",8051,"300 - 1000","23,9 / 41.4","200 ?","2,7 - 3,6","FSK","cc1010","-20 +10","-107 (2,4kbps)","65kHz ?","76,8","2*UART , SPI",14.7456,"Programable Xtal tempcorrection"]
["Chipcon/Texas","cc1020","CC1020-RTB1","N","402 - 470 / 804 - 940","19,9 / 27,1",200,"2,3 - 3,5","OOK/FSK/GFSK","cc1020","-20 +10","-118","12,5kHz","153,6","SPI",14.7456,"Programable Xtal tempcorrection"]
["Chipcon/Texas","cc1021","CC1021-RTB1","N","402 - 470 / 804 - 940","19,9 / 27,1",200,"2,3 - 3.6","OOK/FSK/GFSK","cc1021","-20 +10","-112","50kHz","153,6","SPI",14.7456,"Auto frequence correcton"]
["Chipcon/Texas","cc1100","CC1100-RTY1","N","400 - 464 / 800 - 928","15,6 / 28,8",400,"1,8 - 3,6","GFSK/FSK/OOK/ASK/MSK","cc1100","-30 +10","-110 (1,2kbps)","50kHz","1,2 - 500","SPI",26,"Auto frequence correcton, FIFObuffer"]
["Chipcon/Texas","cc1110","CC1110-RTY1",8051,"315-915","22 / 31","800 / 600","2,0 - 3,6","FSK/GFSK/MSK","cc1110","-30 +10","-109 (10kbps)","50kHz","1,2 - 500","2*USART/SPI",26,"Auto frequence correcton, FIFObuffer"]
["Maxim","Max7030","MAX7030HATJ","N",433.92,"4,3 / 12,4",800,"2,1 - 5,5","ASK","Max7030","10","-113","50kHz?","33 (66 NRZ enc)","3-wire serial","24","50Ohm last"]
["Maxim","Max7032","MAX7032ATJ","N","300 - 450","6,7 / 12,5",800,"2,1 - 5,5","ASK / FSK","Max7032",null,"-110 (FSK)","50kHz?","33 (66 NRZ enc)","3-wire serial"]

{"sheet":"Ordlista","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Regler","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}