(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "AudioJack-CUI-SJ-3523-SMT" (in_bom yes) (on_board yes)
    (property "Reference" "J" (id 0) (at 0 8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "AudioJack-CUI-SJ-3523-SMT" (id 1) (at 0 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "RPi_Pico:CUI_SJ-3523-audio-jack" (id 2) (at 2.54 -6.35 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Jack*" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "AudioJack-CUI-SJ-3523-SMT_0_1"
      (rectangle (start -5.08 -5.08) (end -6.35 -2.54)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type outline))
      )
      (polyline
        (pts
          (xy 0 -2.54)
          (xy 0.635 -3.175)
          (xy 1.27 -2.54)
          (xy 2.54 -2.54)
        )
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -1.905 -2.54)
          (xy -1.27 -3.175)
          (xy -0.635 -2.54)
          (xy -0.635 0)
          (xy 2.54 0)
        )
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 2.54 2.54)
          (xy -2.54 2.54)
          (xy -2.54 -2.54)
          (xy -3.175 -3.175)
          (xy -3.81 -2.54)
        )
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (rectangle (start 2.54 3.81) (end -5.08 -5.08)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "AudioJack-CUI-SJ-3523-SMT_1_1"
      (pin passive line (at 5.08 2.54 180) (length 2.54)
        (name "S" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 5.08 -2.54 180) (length 2.54)
        (name "T" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 5.08 0 180) (length 2.54)
        (name "R" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "NC7WZ16P6X" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -5.08 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "NC7WZ16P6X" (id 1) (at 0 -6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6" (id 2) (at 0 -8.89 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "NC7WZ16P6X_0_1"
      (rectangle (start -6.35 5.08) (end 6.35 -5.08)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 1.27 -2.54)
          (xy 2.54 -2.54)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.27 2.54)
          (xy 2.54 2.54)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -2.54 -2.54)
          (xy -1.27 -2.54)
          (xy -1.27 -1.27)
          (xy 1.27 -2.54)
          (xy -1.27 -3.81)
          (xy -1.27 -2.54)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -2.54 2.54)
          (xy -1.27 2.54)
          (xy -1.27 3.81)
          (xy 1.27 2.54)
          (xy -1.27 1.27)
          (xy -1.27 2.54)
          (xy -2.54 2.54)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
    )
    (symbol "NC7WZ16P6X_1_1"
      (pin input line (at -8.89 2.54 0) (length 2.54)
        (name "A1" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -8.89 0 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -8.89 -2.54 0) (length 2.54)
        (name "A2" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 8.89 -2.54 180) (length 2.54)
        (name "Y2" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 8.89 0 180) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 8.89 2.54 180) (length 2.54)
        (name "Y1" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Pico" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -13.97 27.94 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "Pico" (id 1) (at 0 19.05 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "RPi_Pico:RPi_Pico_SMD_TH" (id 2) (at 0 0 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "Pico_0_0"
      (text "Raspberry Pi" (at 0 21.59 0)
        (effects (font (size 1.27 1.27)))
      )
    )
    (symbol "Pico_0_1"
      (rectangle (start -15.24 26.67) (end 15.24 -26.67)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "Pico_1_1"
      (pin bidirectional line (at -17.78 24.13 0) (length 2.54)
        (name "GPIO0" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 1.27 0) (length 2.54)
        (name "GPIO7" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 -1.27 0) (length 2.54)
        (name "GPIO8" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 -3.81 0) (length 2.54)
        (name "GPIO9" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -17.78 -6.35 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 -8.89 0) (length 2.54)
        (name "GPIO10" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 -11.43 0) (length 2.54)
        (name "GPIO11" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 -13.97 0) (length 2.54)
        (name "GPIO12" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 -16.51 0) (length 2.54)
        (name "GPIO13" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -17.78 -19.05 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 -21.59 0) (length 2.54)
        (name "GPIO14" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 21.59 0) (length 2.54)
        (name "GPIO1" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 -24.13 0) (length 2.54)
        (name "GPIO15" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -24.13 180) (length 2.54)
        (name "GPIO16" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -21.59 180) (length 2.54)
        (name "GPIO17" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 17.78 -19.05 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -16.51 180) (length 2.54)
        (name "GPIO18" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -13.97 180) (length 2.54)
        (name "GPIO19" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -11.43 180) (length 2.54)
        (name "GPIO20" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -8.89 180) (length 2.54)
        (name "GPIO21" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 17.78 -6.35 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -3.81 180) (length 2.54)
        (name "GPIO22" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -17.78 19.05 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 17.78 -1.27 180) (length 2.54)
        (name "RUN" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 1.27 180) (length 2.54)
        (name "GPIO26_ADC0" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 3.81 180) (length 2.54)
        (name "GPIO27_ADC1" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 17.78 6.35 180) (length 2.54)
        (name "AGND" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 8.89 180) (length 2.54)
        (name "GPIO28_ADC2" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line (at 17.78 11.43 180) (length 2.54)
        (name "ADC_VREF" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line (at 17.78 13.97 180) (length 2.54)
        (name "3V3" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 17.78 16.51 180) (length 2.54)
        (name "3V3_EN" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 19.05 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line (at 17.78 21.59 180) (length 2.54)
        (name "VSYS" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 16.51 0) (length 2.54)
        (name "GPIO2" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line (at 17.78 24.13 180) (length 2.54)
        (name "VBUS" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -2.54 -29.21 90) (length 2.54)
        (name "SWCLK" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -29.21 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 2.54 -29.21 90) (length 2.54)
        (name "SWDIO" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 13.97 0) (length 2.54)
        (name "GPIO3" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 11.43 0) (length 2.54)
        (name "GPIO4" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 8.89 0) (length 2.54)
        (name "GPIO5" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -17.78 6.35 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 3.81 0) (length 2.54)
        (name "GPIO6" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "PicoW" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -13.97 27.94 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "PicoW" (id 1) (at 0 19.05 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "RPi_PicoW:RPi_Pico_SMD_TH" (id 2) (at 0 0 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "PicoW_0_0"
      (text "Raspberry Pi" (at 0 21.59 0)
        (effects (font (size 1.27 1.27)))
      )
    )
    (symbol "PicoW_0_1"
      (rectangle (start -15.24 26.67) (end 15.24 -26.67)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "PicoW_1_1"
      (pin bidirectional line (at -17.78 24.13 0) (length 2.54)
        (name "GPIO0" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 1.27 0) (length 2.54)
        (name "GPIO7" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 -1.27 0) (length 2.54)
        (name "GPIO8" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 -3.81 0) (length 2.54)
        (name "GPIO9" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -17.78 -6.35 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 -8.89 0) (length 2.54)
        (name "GPIO10" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 -11.43 0) (length 2.54)
        (name "GPIO11" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 -13.97 0) (length 2.54)
        (name "GPIO12" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 -16.51 0) (length 2.54)
        (name "GPIO13" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -17.78 -19.05 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 -21.59 0) (length 2.54)
        (name "GPIO14" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 21.59 0) (length 2.54)
        (name "GPIO1" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 -24.13 0) (length 2.54)
        (name "GPIO15" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -24.13 180) (length 2.54)
        (name "GPIO16" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -21.59 180) (length 2.54)
        (name "GPIO17" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 17.78 -19.05 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -16.51 180) (length 2.54)
        (name "GPIO18" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -13.97 180) (length 2.54)
        (name "GPIO19" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -11.43 180) (length 2.54)
        (name "GPIO20" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -8.89 180) (length 2.54)
        (name "GPIO21" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 17.78 -6.35 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -3.81 180) (length 2.54)
        (name "GPIO22" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -17.78 19.05 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 17.78 -1.27 180) (length 2.54)
        (name "RUN" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 1.27 180) (length 2.54)
        (name "GPIO26_ADC0" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 3.81 180) (length 2.54)
        (name "GPIO27_ADC1" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 17.78 6.35 180) (length 2.54)
        (name "AGND" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 8.89 180) (length 2.54)
        (name "GPIO28_ADC2" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line (at 17.78 11.43 180) (length 2.54)
        (name "ADC_VREF" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line (at 17.78 13.97 180) (length 2.54)
        (name "3V3" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 17.78 16.51 180) (length 2.54)
        (name "3V3_EN" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 19.05 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line (at 17.78 21.59 180) (length 2.54)
        (name "VSYS" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 16.51 0) (length 2.54)
        (name "GPIO2" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line (at 17.78 24.13 180) (length 2.54)
        (name "VBUS" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -2.54 -29.21 90) (length 2.54)
        (name "SWCLK" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -29.21 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 2.54 -29.21 90) (length 2.54)
        (name "SWDIO" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 13.97 0) (length 2.54)
        (name "GPIO3" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 11.43 0) (length 2.54)
        (name "GPIO4" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 8.89 0) (length 2.54)
        (name "GPIO5" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -17.78 6.35 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 3.81 0) (length 2.54)
        (name "GPIO6" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
