(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "+3.3V-power" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
    (property "Reference" "#PWR" (id 0) (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Value" "+3.3V-power" (id 1) (at 0 3.556 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "+3.3V-power_0_1"
      (polyline
        (pts
          (xy -0.762 1.27)
          (xy 0 2.54)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 0)
          (xy 0 2.54)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 2.54)
          (xy 0.762 1.27)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
    )
    (symbol "+3.3V-power_1_1"
      (pin power_in line (at 0 0 90) (length 0) hide
        (name "+3V3" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Teensy3.2-Teensy" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 39.37 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Value" "Teensy3.2-Teensy" (id 1) (at 0 -39.37 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Footprint" "" (id 2) (at 0 -19.05 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Datasheet" "" (id 3) (at 0 -19.05 0)
      (effects (font (size 1.524 1.524)))
    )
    (symbol "Teensy3.2-Teensy_0_0"
      (text "3.6V to 6.0V" (at 8.89 -24.13 0)
        (effects (font (size 1.27 1.27)))
      )
      (text "max 250mA" (at 7.62 -29.21 0)
        (effects (font (size 1.27 1.27)))
      )
    )
    (symbol "Teensy3.2-Teensy_0_1"
      (rectangle (start -20.32 -36.83) (end 20.32 36.83)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
    )
    (symbol "Teensy3.2-Teensy_1_1"
      (pin power_in line (at -25.4 34.29 0) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -25.4 11.43 0) (length 5.08)
        (name "8_TX3_DIN" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -25.4 8.89 0) (length 5.08)
        (name "9_RX2_CS_PWM" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -25.4 6.35 0) (length 5.08)
        (name "10_TX2_CS_PWM" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -25.4 3.81 0) (length 5.08)
        (name "11_DOUT" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -25.4 1.27 0) (length 5.08)
        (name "12_DIN" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -25.4 -1.27 0) (length 5.08)
        (name "VBat" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -25.4 -3.81 0) (length 5.08)
        (name "3.3V" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -25.4 -6.35 0) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -25.4 -8.89 0) (length 5.08)
        (name "Program" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -25.4 -11.43 0) (length 5.08)
        (name "A14/DAC" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -25.4 31.75 0) (length 5.08)
        (name "0_RX1_Touch" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -25.4 -13.97 0) (length 5.08)
        (name "13_LED_SCK" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -25.4 -16.51 0) (length 5.08)
        (name "14_A0_SCK" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -25.4 -19.05 0) (length 5.08)
        (name "15_A1_CS_Touch" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -25.4 -21.59 0) (length 5.08)
        (name "16_A2_SCL0_Touch" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -25.4 -24.13 0) (length 5.08)
        (name "17_A3_SDA0_Touch" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -25.4 -26.67 0) (length 5.08)
        (name "18_A4_SDA0_Touch" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -25.4 -29.21 0) (length 5.08)
        (name "19_A5_SCL0_Touch" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -25.4 -31.75 0) (length 5.08)
        (name "20_A6_CS_PWM" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -25.4 -34.29 0) (length 5.08)
        (name "21_A7_RX1_CS_PWM" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 -34.29 180) (length 5.08)
        (name "22_A8_Touch_PWM" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -25.4 29.21 0) (length 5.08)
        (name "1_TX1_Touch" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 -31.75 180) (length 5.08)
        (name "23_A9_Touch_PWM" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 25.4 -29.21 180) (length 5.08)
        (name "3.3V" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 25.4 -26.67 180) (length 5.08)
        (name "AGND" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 25.4 -24.13 180) (length 5.08)
        (name "Vin" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 25.4 -21.59 180) (length 5.08)
        (name "VUSB" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 25.4 -19.05 180) (length 5.08)
        (name "AREF" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 -16.51 180) (length 5.08)
        (name "A10" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 -13.97 180) (length 5.08)
        (name "A11" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -25.4 26.67 0) (length 5.08)
        (name "2" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -25.4 24.13 0) (length 5.08)
        (name "3_TX_PWM" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -25.4 21.59 0) (length 5.08)
        (name "4_RX_PWM" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -25.4 19.05 0) (length 5.08)
        (name "5_TX1_PWM" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -25.4 16.51 0) (length 5.08)
        (name "6_PWM" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -25.4 13.97 0) (length 5.08)
        (name "7_RX3_DOUT" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 -1.27 180) (length 5.08)
        (name "24" (effects (font (size 1.27 1.27))))
        (number "~" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 1.27 180) (length 5.08)
        (name "25_Touch_PWM" (effects (font (size 1.27 1.27))))
        (number "~" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 3.81 180) (length 5.08)
        (name "26_A15_RX2" (effects (font (size 1.27 1.27))))
        (number "~" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 6.35 180) (length 5.08)
        (name "27_A16" (effects (font (size 1.27 1.27))))
        (number "~" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 8.89 180) (length 5.08)
        (name "28_A17" (effects (font (size 1.27 1.27))))
        (number "~" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 11.43 180) (length 5.08)
        (name "29_A18_SCL1" (effects (font (size 1.27 1.27))))
        (number "~" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 25.4 24.13 180) (length 5.08)
        (name "3.3V" (effects (font (size 1.27 1.27))))
        (number "~" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 13.97 180) (length 5.08)
        (name "30_A19_SDA1" (effects (font (size 1.27 1.27))))
        (number "~" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 16.51 180) (length 5.08)
        (name "31_A20_TX2" (effects (font (size 1.27 1.27))))
        (number "~" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 19.05 180) (length 5.08)
        (name "32_Touch_PWM" (effects (font (size 1.27 1.27))))
        (number "~" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 21.59 180) (length 5.08)
        (name "33_Touch" (effects (font (size 1.27 1.27))))
        (number "~" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 -6.35 180) (length 5.08)
        (name "A12" (effects (font (size 1.27 1.27))))
        (number "~" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 26.67 180) (length 5.08)
        (name "A13" (effects (font (size 1.27 1.27))))
        (number "~" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 31.75 180) (length 5.08)
        (name "D+" (effects (font (size 1.27 1.27))))
        (number "~" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 34.29 180) (length 5.08)
        (name "D-" (effects (font (size 1.27 1.27))))
        (number "~" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 25.4 -3.81 180) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "~" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 25.4 29.21 180) (length 5.08)
        (name "Reset" (effects (font (size 1.27 1.27))))
        (number "~" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
