(export (version D)
  (design
    (source D:\Projects\cmdr_system\kicad\cmdr_mainboard\cmdr_mainboard.sch)
    (date "02/07/20 12:05:52")
    (tool "Eeschema (5.1.5)-3")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title "CMDR Mainboard")
        (company CMtec)
        (rev 01)
        (date 2020-02-04)
        (source cmdr_mainboard.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref U1)
      (value Teensy3.2)
      (footprint cmdr_mainboard:Teensy30_31_32_LC_CM)
      (libsource (lib cmdr_mainboard-rescue) (part Teensy3.2-Teensy) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E395E08))
    (comp (ref J8)
      (value Base)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x04) (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E39FC27))
    (comp (ref R1)
      (value 0)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E39840D))
    (comp (ref R2)
      (value 0)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E39CACF))
    (comp (ref R5)
      (value 220)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E39D334))
    (comp (ref R6)
      (value 220)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E39DA65))
    (comp (ref R3)
      (value 220)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E39DCA7))
    (comp (ref R4)
      (value 220)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E39E29C))
    (comp (ref R11)
      (value 15k)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E3E50F7))
    (comp (ref R12)
      (value 15k)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E3E5594))
    (comp (ref R9)
      (value 10k)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E3E58FD))
    (comp (ref R7)
      (value 10k)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E3E5EAC))
    (comp (ref R15)
      (value 0)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E3E60C5))
    (comp (ref R17)
      (value 0)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E3E648F))
    (comp (ref R13)
      (value 15k)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E40FFB2))
    (comp (ref R14)
      (value 15k)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E40FFBC))
    (comp (ref R10)
      (value 10k)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E40FFC6))
    (comp (ref R8)
      (value 10k)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E40FFD0))
    (comp (ref R18)
      (value 0)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E40FFE4))
    (comp (ref R16)
      (value 0)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E40FFDA))
    (comp (ref J10)
      (value POL-2119)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x03) (description "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E54EFBB))
    (comp (ref U2)
      (value 74LVC1G125)
      (footprint Package_TO_SOT_SMD:SOT-23-5_HandSoldering)
      (datasheet http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf)
      (libsource (lib 74xGxx) (part 74LVC1G125) (description "Single Buffer Gate Tri-State, Low-Voltage CMOS"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E3D1E79))
    (comp (ref U3)
      (value 74LVC1G125)
      (footprint Package_TO_SOT_SMD:SOT-23-5_HandSoldering)
      (datasheet http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf)
      (libsource (lib 74xGxx) (part 74LVC1G125) (description "Single Buffer Gate Tri-State, Low-Voltage CMOS"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E3D90B8))
    (comp (ref H4)
      (value MountingHole)
      (footprint MountingHole:MountingHole_2.2mm_M2)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E42C524))
    (comp (ref H3)
      (value MountingHole)
      (footprint MountingHole:MountingHole_2.2mm_M2)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E42DBD8))
    (comp (ref H2)
      (value MountingHole)
      (footprint MountingHole:MountingHole_2.2mm_M2)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E438FA4))
    (comp (ref H1)
      (value MountingHole)
      (footprint MountingHole:MountingHole_2.2mm_M2)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E439507))
    (comp (ref J6)
      (value Handle)
      (footprint Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x04_Odd_Even) (description "Generic connector, double row, 02x04, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E3AEB11))
    (comp (ref C2)
      (value C)
      (footprint Capacitor_SMD:C_1210_3225Metric_Pad1.42x2.65mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E3B10D6))
    (comp (ref C1)
      (value C)
      (footprint Capacitor_SMD:C_1210_3225Metric_Pad1.42x2.65mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E3B0AC0))
    (comp (ref J4)
      (value Keys)
      (footprint Connector_PinHeader_2.54mm:PinHeader_2x06_P2.54mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x06_Odd_Even) (description "Generic connector, double row, 02x06, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E59A0DF))
    (comp (ref J2)
      (value RJ45)
      (footprint Connector_RJ:RJ45_Amphenol_54602-x08_Horizontal)
      (datasheet ~)
      (libsource (lib Connector) (part RJ45) (description "RJ connector, 8P8C (8 positions 8 connected)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E399245))
    (comp (ref J1)
      (value RJ45)
      (footprint Connector_RJ:RJ45_Amphenol_54602-x08_Horizontal)
      (datasheet ~)
      (libsource (lib Connector) (part RJ45) (description "RJ connector, 8P8C (8 positions 8 connected)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E39B2A1))
    (comp (ref L1)
      (value Bead)
      (footprint Inductor_SMD:L_1206_3216Metric)
      (datasheet ~)
      (libsource (lib Device) (part L) (description Inductor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E48E5E4))
    (comp (ref L2)
      (value Bead)
      (footprint Inductor_SMD:L_1206_3216Metric)
      (datasheet ~)
      (libsource (lib Device) (part L) (description Inductor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E4A66E5))
    (comp (ref H5)
      (value MountingHole)
      (footprint MountingHole:MountingHole_2.2mm_M2)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E576885))
    (comp (ref J5)
      (value DotStar)
      (footprint Connector_PinHeader_2.54mm:PinHeader_2x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x02_Odd_Even) (description "Generic connector, double row, 02x02, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E576B9E))
    (comp (ref J7)
      (value "DotStar Mounting only")
      (footprint Connector_PinHeader_2.54mm:PinHeader_2x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x02_Odd_Even) (description "Generic connector, double row, 02x02, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E5FE8ED))
    (comp (ref J3)
      (value D-)
      (footprint Connector_Wire:SolderWirePad_1x01_Drill0.8mm)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x01) (description "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E3DB4BB))
    (comp (ref J9)
      (value D+)
      (footprint Connector_Wire:SolderWirePad_1x01_Drill0.8mm)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x01) (description "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E3DC035)))
  (libparts
    (libpart (lib 74xGxx) (part 74LVC1G125)
      (aliases
        (alias 74AHC1G125)
        (alias 74AHCT1G125)
        (alias 74AUC1G125)
        (alias 74AUP1G125))
      (description "Single Buffer Gate Tri-State, Low-Voltage CMOS")
      (docs http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf)
      (footprints
        (fp SOT*)
        (fp SG-*))
      (fields
        (field (name Reference) U)
        (field (name Value) 74LVC1G125))
      (pins
        (pin (num 1) (name ~) (type input))
        (pin (num 2) (name ~) (type input))
        (pin (num 3) (name GND) (type power_in))
        (pin (num 4) (name ~) (type 3state))
        (pin (num 5) (name VCC) (type power_in))))
    (libpart (lib Connector) (part 8P8C)
      (aliases
        (alias RJ31)
        (alias RJ32)
        (alias RJ33)
        (alias RJ34)
        (alias RJ35)
        (alias RJ41)
        (alias RJ45)
        (alias RJ49)
        (alias RJ61))
      (description "RJ connector, 8P8C (8 positions 8 connected), RJ31/RJ32/RJ33/RJ34/RJ35/RJ41/RJ45/RJ49/RJ61")
      (docs ~)
      (footprints
        (fp 8P8C*)
        (fp RJ31*)
        (fp RJ32*)
        (fp RJ33*)
        (fp RJ34*)
        (fp RJ35*)
        (fp RJ41*)
        (fp RJ45*)
        (fp RJ49*)
        (fp RJ61*))
      (fields
        (field (name Reference) J)
        (field (name Value) 8P8C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))
        (pin (num 7) (name ~) (type passive))
        (pin (num 8) (name ~) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_01x01)
      (description "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x01))
      (pins
        (pin (num 1) (name Pin_1) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_01x03)
      (description "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x03))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_01x04)
      (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x04))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_02x02_Odd_Even)
      (description "Generic connector, double row, 02x02, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x02_Odd_Even))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_02x04_Odd_Even)
      (description "Generic connector, double row, 02x04, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x04_Odd_Even))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_02x06_Odd_Even)
      (description "Generic connector, double row, 02x06, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x06_Odd_Even))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))))
    (libpart (lib Device) (part C)
      (description "Unpolarized capacitor")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part L)
      (description Inductor)
      (docs ~)
      (footprints
        (fp Choke_*)
        (fp *Coil*)
        (fp Inductor_*)
        (fp L_*))
      (fields
        (field (name Reference) L)
        (field (name Value) L))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib Device) (part R)
      (description Resistor)
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Mechanical) (part MountingHole)
      (description "Mounting Hole without connection")
      (docs ~)
      (footprints
        (fp MountingHole*))
      (fields
        (field (name Reference) H)
        (field (name Value) MountingHole)))
    (libpart (lib cmdr_mainboard-rescue) (part Teensy3.2-Teensy)
      (fields
        (field (name Reference) U)
        (field (name Value) Teensy3.2-Teensy))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name 0_RX1_Touch) (type BiDi))
        (pin (num 3) (name 1_TX1_Touch) (type BiDi))
        (pin (num 4) (name 2) (type BiDi))
        (pin (num 5) (name 3_TX_PWM) (type BiDi))
        (pin (num 6) (name 4_RX_PWM) (type BiDi))
        (pin (num 7) (name 5_TX1_PWM) (type BiDi))
        (pin (num 8) (name 6_PWM) (type BiDi))
        (pin (num 9) (name 7_RX3_DOUT) (type BiDi))
        (pin (num 10) (name 8_TX3_DIN) (type BiDi))
        (pin (num 11) (name 9_RX2_CS_PWM) (type BiDi))
        (pin (num 12) (name 10_TX2_CS_PWM) (type BiDi))
        (pin (num 13) (name 11_DOUT) (type BiDi))
        (pin (num 14) (name 12_DIN) (type BiDi))
        (pin (num 15) (name VBat) (type power_in))
        (pin (num 16) (name 3.3V) (type power_out))
        (pin (num 17) (name GND) (type power_in))
        (pin (num 18) (name Program) (type input))
        (pin (num 19) (name A14/DAC) (type BiDi))
        (pin (num 20) (name 13_LED_SCK) (type BiDi))
        (pin (num 21) (name 14_A0_SCK) (type BiDi))
        (pin (num 22) (name 15_A1_CS_Touch) (type BiDi))
        (pin (num 23) (name 16_A2_SCL0_Touch) (type BiDi))
        (pin (num 24) (name 17_A3_SDA0_Touch) (type BiDi))
        (pin (num 25) (name 18_A4_SDA0_Touch) (type BiDi))
        (pin (num 26) (name 19_A5_SCL0_Touch) (type BiDi))
        (pin (num 27) (name 20_A6_CS_PWM) (type BiDi))
        (pin (num 28) (name 21_A7_RX1_CS_PWM) (type BiDi))
        (pin (num 29) (name 22_A8_Touch_PWM) (type BiDi))
        (pin (num 30) (name 23_A9_Touch_PWM) (type BiDi))
        (pin (num 31) (name 3.3V) (type power_out))
        (pin (num 32) (name AGND) (type power_out))
        (pin (num 33) (name Vin) (type power_in))
        (pin (num 34) (name VUSB) (type power_in))
        (pin (num 35) (name AREF) (type input))
        (pin (num 36) (name A10) (type BiDi))
        (pin (num 37) (name A11) (type BiDi))
        (pin (num ~) (name Reset) (type input)))))
  (libraries
    (library (logical 74xGxx)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/74xGxx.lib"))
    (library (logical Connector)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Connector.lib"))
    (library (logical Connector_Generic)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Connector_Generic.lib"))
    (library (logical Device)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Device.lib"))
    (library (logical Mechanical)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Mechanical.lib"))
    (library (logical cmdr_mainboard-rescue)
      (uri D:\Projects\cmdr_system\kicad\cmdr_mainboard/cmdr_mainboard-rescue.lib)))
  (nets
    (net (code 1) (name SCL)
      (node (ref U1) (pin 26))
      (node (ref J6) (pin 6)))
    (net (code 2) (name SDA)
      (node (ref J6) (pin 4))
      (node (ref U1) (pin 25)))
    (net (code 3) (name "Net-(J6-Pad1)")
      (node (ref R16) (pin 2))
      (node (ref R18) (pin 2))
      (node (ref J6) (pin 1)))
    (net (code 4) (name VBUS)
      (node (ref J10) (pin 1))
      (node (ref U1) (pin 33))
      (node (ref U3) (pin 5))
      (node (ref U2) (pin 5))
      (node (ref J5) (pin 1))
      (node (ref J1) (pin 1))
      (node (ref J2) (pin 1)))
    (net (code 5) (name "Net-(J4-Pad1)")
      (node (ref J4) (pin 1)))
    (net (code 6) (name "Net-(J4-Pad9)")
      (node (ref J4) (pin 9))
      (node (ref U1) (pin 7)))
    (net (code 7) (name "Net-(J4-Pad7)")
      (node (ref J4) (pin 7))
      (node (ref U1) (pin 6)))
    (net (code 8) (name "Net-(J4-Pad10)")
      (node (ref U1) (pin 21))
      (node (ref J4) (pin 10)))
    (net (code 9) (name "Net-(U1-Pad30)")
      (node (ref U3) (pin 2))
      (node (ref U1) (pin 30)))
    (net (code 10) (name "Net-(J5-Pad2)")
      (node (ref J5) (pin 2))
      (node (ref U2) (pin 4)))
    (net (code 11) (name "Net-(J1-Pad5)")
      (node (ref J1) (pin 5))
      (node (ref J2) (pin 5)))
    (net (code 12) (name "Net-(J1-Pad6)")
      (node (ref J2) (pin 6))
      (node (ref J1) (pin 6)))
    (net (code 13) (name "Net-(U1-Pad29)")
      (node (ref U1) (pin 29))
      (node (ref U2) (pin 2)))
    (net (code 14) (name "Net-(J5-Pad4)")
      (node (ref J5) (pin 4))
      (node (ref U3) (pin 4)))
    (net (code 15) (name "Net-(J4-Pad5)")
      (node (ref J4) (pin 5))
      (node (ref U1) (pin 5)))
    (net (code 16) (name +5V)
      (node (ref L1) (pin 2))
      (node (ref R18) (pin 1))
      (node (ref R17) (pin 1)))
    (net (code 17) (name GND)
      (node (ref J5) (pin 3))
      (node (ref C1) (pin 2))
      (node (ref J10) (pin 2))
      (node (ref L2) (pin 1))
      (node (ref J1) (pin 2))
      (node (ref J6) (pin 8))
      (node (ref J2) (pin 2))
      (node (ref U1) (pin 1))
      (node (ref C2) (pin 2))
      (node (ref U3) (pin 3))
      (node (ref U3) (pin 1))
      (node (ref U2) (pin 3))
      (node (ref U2) (pin 1)))
    (net (code 18) (name /5VR)
      (node (ref L1) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref J10) (pin 3))
      (node (ref C1) (pin 1)))
    (net (code 19) (name "Net-(J7-Pad4)")
      (node (ref J7) (pin 4)))
    (net (code 20) (name "Net-(J7-Pad2)")
      (node (ref J7) (pin 2)))
    (net (code 21) (name "Net-(J7-Pad3)")
      (node (ref J7) (pin 3)))
    (net (code 22) (name "Net-(J7-Pad1)")
      (node (ref J7) (pin 1)))
    (net (code 23) (name "Net-(J4-Pad3)")
      (node (ref J4) (pin 3))
      (node (ref U1) (pin 4)))
    (net (code 24) (name "Net-(J2-Pad4)")
      (node (ref J2) (pin 4)))
    (net (code 25) (name "Net-(J2-Pad3)")
      (node (ref J2) (pin 3)))
    (net (code 26) (name TX2)
      (node (ref R6) (pin 2))
      (node (ref U1) (pin 10)))
    (net (code 27) (name RX2)
      (node (ref U1) (pin 9))
      (node (ref R5) (pin 2)))
    (net (code 28) (name /D-)
      (node (ref J1) (pin 4))
      (node (ref J3) (pin 1)))
    (net (code 29) (name /D+)
      (node (ref J1) (pin 3))
      (node (ref J9) (pin 1)))
    (net (code 30) (name "Net-(J4-Pad11)")
      (node (ref J4) (pin 11))
      (node (ref U1) (pin 8)))
    (net (code 31) (name "Net-(J1-Pad8)")
      (node (ref R4) (pin 1))
      (node (ref J1) (pin 8))
      (node (ref R2) (pin 1)))
    (net (code 32) (name "Net-(J2-Pad8)")
      (node (ref J2) (pin 8))
      (node (ref R3) (pin 1))
      (node (ref R2) (pin 2)))
    (net (code 33) (name "Net-(R4-Pad2)")
      (node (ref R4) (pin 2))
      (node (ref U1) (pin 3)))
    (net (code 34) (name "Net-(J2-Pad7)")
      (node (ref J2) (pin 7))
      (node (ref R5) (pin 1))
      (node (ref R1) (pin 2)))
    (net (code 35) (name "Net-(J1-Pad7)")
      (node (ref J1) (pin 7))
      (node (ref R1) (pin 1))
      (node (ref R6) (pin 1)))
    (net (code 36) (name GNDA)
      (node (ref R7) (pin 2))
      (node (ref R10) (pin 2))
      (node (ref J6) (pin 7))
      (node (ref R9) (pin 2))
      (node (ref R8) (pin 2))
      (node (ref J8) (pin 4))
      (node (ref U1) (pin 32))
      (node (ref L2) (pin 2)))
    (net (code 37) (name "Net-(R3-Pad2)")
      (node (ref R3) (pin 2))
      (node (ref U1) (pin 2)))
    (net (code 38) (name "Net-(J4-Pad12)")
      (node (ref U1) (pin 22))
      (node (ref J4) (pin 12)))
    (net (code 39) (name "Net-(U1-Pad34)")
      (node (ref U1) (pin 34)))
    (net (code 40) (name "Net-(U1-Pad35)")
      (node (ref U1) (pin 35)))
    (net (code 41) (name "Net-(U1-Pad20)")
      (node (ref U1) (pin 20)))
    (net (code 42) (name "Net-(U1-Pad19)")
      (node (ref U1) (pin 19)))
    (net (code 43) (name "Net-(U1-Pad18)")
      (node (ref U1) (pin 18)))
    (net (code 44) (name "Net-(U1-Pad17)")
      (node (ref U1) (pin 17)))
    (net (code 45) (name "Net-(U1-Pad16)")
      (node (ref U1) (pin 16)))
    (net (code 46) (name "Net-(U1-Pad15)")
      (node (ref U1) (pin 15)))
    (net (code 47) (name "Net-(J4-Pad8)")
      (node (ref J4) (pin 8))
      (node (ref U1) (pin 14)))
    (net (code 48) (name "Net-(J4-Pad6)")
      (node (ref U1) (pin 13))
      (node (ref J4) (pin 6)))
    (net (code 49) (name "Net-(J4-Pad4)")
      (node (ref J4) (pin 4))
      (node (ref U1) (pin 12)))
    (net (code 50) (name "Net-(J4-Pad2)")
      (node (ref J4) (pin 2))
      (node (ref U1) (pin 11)))
    (net (code 51) (name "Net-(U1-Pad~)")
      (node (ref U1) (pin ~)))
    (net (code 52) (name "Net-(J8-Pad2)")
      (node (ref J8) (pin 2))
      (node (ref R11) (pin 2)))
    (net (code 53) (name "Net-(J8-Pad1)")
      (node (ref R17) (pin 2))
      (node (ref R15) (pin 2))
      (node (ref J8) (pin 1)))
    (net (code 54) (name "Net-(U1-Pad~)")
      (node (ref U1) (pin ~)))
    (net (code 55) (name "Net-(U1-Pad~)")
      (node (ref U1) (pin ~)))
    (net (code 56) (name "Net-(U1-Pad~)")
      (node (ref U1) (pin ~)))
    (net (code 57) (name "Net-(U1-Pad~)")
      (node (ref U1) (pin ~)))
    (net (code 58) (name "Net-(U1-Pad~)")
      (node (ref U1) (pin ~)))
    (net (code 59) (name "Net-(U1-Pad~)")
      (node (ref U1) (pin ~)))
    (net (code 60) (name "Net-(U1-Pad~)")
      (node (ref U1) (pin ~)))
    (net (code 61) (name "Net-(U1-Pad~)")
      (node (ref U1) (pin ~)))
    (net (code 62) (name "Net-(U1-Pad~)")
      (node (ref U1) (pin ~)))
    (net (code 63) (name "Net-(U1-Pad~)")
      (node (ref U1) (pin ~)))
    (net (code 64) (name "Net-(U1-Pad~)")
      (node (ref U1) (pin ~)))
    (net (code 65) (name "Net-(U1-Pad~)")
      (node (ref U1) (pin ~)))
    (net (code 66) (name "Net-(U1-Pad~)")
      (node (ref U1) (pin ~)))
    (net (code 67) (name "Net-(U1-Pad~)")
      (node (ref U1) (pin ~)))
    (net (code 68) (name "Net-(U1-Pad~)")
      (node (ref U1) (pin ~)))
    (net (code 69) (name "Net-(U1-Pad~)")
      (node (ref U1) (pin ~)))
    (net (code 70) (name "Net-(U1-Pad37)")
      (node (ref U1) (pin 37)))
    (net (code 71) (name "Net-(U1-Pad36)")
      (node (ref U1) (pin 36)))
    (net (code 72) (name "Net-(J6-Pad5)")
      (node (ref J6) (pin 5))
      (node (ref R14) (pin 2)))
    (net (code 73) (name Y2)
      (node (ref U1) (pin 28))
      (node (ref R10) (pin 1))
      (node (ref R14) (pin 1)))
    (net (code 74) (name "Net-(J6-Pad3)")
      (node (ref R13) (pin 2))
      (node (ref J6) (pin 3)))
    (net (code 75) (name X2)
      (node (ref R8) (pin 1))
      (node (ref U1) (pin 27))
      (node (ref R13) (pin 1)))
    (net (code 76) (name +3V3)
      (node (ref J6) (pin 2))
      (node (ref R15) (pin 1))
      (node (ref U1) (pin 31))
      (node (ref R16) (pin 1)))
    (net (code 77) (name Y1)
      (node (ref R12) (pin 1))
      (node (ref R9) (pin 1))
      (node (ref U1) (pin 24)))
    (net (code 78) (name X1)
      (node (ref R7) (pin 1))
      (node (ref R11) (pin 1))
      (node (ref U1) (pin 23)))
    (net (code 79) (name "Net-(J8-Pad3)")
      (node (ref J8) (pin 3))
      (node (ref R12) (pin 2)))))